A · Results — populated (inc. 8888 stress row)
Results
MIL
0.1 MRAD
6.5CM ELD-M 140gr
⚠ G1 BC — predictions degrade beyond 400 yd. Enter DOPE to correct.
Fire Solution
500 yd
+8.4MIL
> 2.1
84 clicks
SPIN DRIFT +0.03 CORIOLIS +0.002
4 / 6 ON LABEL
Dist
Elev
Wind
Clks
✓
8888
−88.8
>88.8
8888
100
+1.2
> 0.4
12
500
+8.4
> 2.1
84
SPIN DRIFT +0.03 · CORIOLIS +0.002
700
−12.1
> 3.0
121
B · Results — empty
Results
MIL
0.1 MRAD
No ammo selected
Awaiting Data
Select ammo and add output distances to generate your fire solution.
C · DOPE — populated (inc. 8888 stress entry)
ScopeDOPE
Ammo
6.5 Creedmoor Hornady ELD-M 140gr
MV 2710 fps · G7 0.301
Known DOPE
01
Dist
100 yd
Adj
+1.2
88
Dist
8888 yd
Adj
−88.8
03
Dist
500 yd
Adj
+8.4
New dist
yd
Adj
mil
D · DOPE — no entries
ScopeDOPE
Ammo
No ammo selected
Known DOPE
+
No confirmed impacts
Add 3 or more range impacts to build your ballistic curve.
Dist
yd
Adj
mil
E · Basic Settings (+25%)
Settings
Adjustment Units
MIL
Milliradians — 1 decimal place (e.g. 3.5)
MOA
MOA — 2 decimal places (e.g. 12.50)
Click Value
Must match your scope's turret denomination
0.1 MRAD
Most common
0.05 MRAD
Measurement System
US Customary
ft, °F, inHg, mph
Metric
m, °C, hPa, km/h
Override individual units in Advanced Settings → Measurement Units.
Label Format
Small
Medium
Large
Portrait
48 mm × 76 mm — 1 column, max 8
Landscape 2 col
76 mm × 48 mm — 2 columns, max 8
Advanced
About
ScopeDOPE
Version 0.9.6-beta4
F · Advanced Settings (+25%)
Advanced Settings
Ballistics Engine
Use Real DOPE Data
Blending your confirmed range data with physics
Corrections
Coriolis Effect
Earth-rotation correction for elevation and windage
Latitude captured from location services only. Never stored remotely or transmitted.
Latitude: 41.88° N
Measurement Units
Per-field overrides. Changing Measurement System resets all fields to system defaults.
Altitude
ft
m
Temperature
°F
°C
K
Kelvin — absolute temperature scale
Pressure
inHg
Inches of mercury — US standard
hPa
Hectopascal — international standard
mbar
mmHg
kPa
Wind Speed
mph
Miles per hour — US standard
km/h
m/s
Scientific / ballistics
kts
Label Appearance
Gridlines
Row separators and column divider visible
Color Mode
Semantic: blue dist, green/red elev, amber wind
Elevation Symbol
+3.5 / −3.5
Default
↑3.5 / ↓3.5
Weather Sensor
WeatherFlow Tactical Recommended
Bluetooth — wind, temp, humidity, pressure, compass
BTMETER BT-100
Bluetooth — wind speed + temperature
Shared Mode
Auto-disconnect after capturing conditions
Printer
Shared Mode
Prints then auto-disconnects — ready for next user
Known Printers
Range Printer B1
Niimbot B1 · AA:BB:CC:DD
G · Splash Screen
BETA
Scope D
PE
Cold Bore Ballistics
v0.9.6-beta4
Precision's NEW Best Friend!
H · Send Feedback
Send Feedback
Category
Bug Report
Feature Request
General
Your Feedback
Device Info
ScopeDOPE v0.9.6-beta4
Android 14 · API 34
Pixel 8 Pro
Included automatically to help us diagnose issues.
Sends to feedback@scope-dope.com
I · Contact Support
Contact Support
Issue Type
Ballistics
Printing
Sensors
Other
Describe Your Issue
Steps to Reproduce
Device Info
ScopeDOPE v0.9.6-beta4
Android 14 · API 34
Pixel 8 Pro
Sends to support@scope-dope.com